**INSTALLATION INSTRUCTIONS FOR LED REMOTE HEAD**

**LED REMOTE HEAD**

**READ AND FOLLOW ALL SAFETY INSTRUCTIONS**

When using electrical,basic safety precautions should always be followed including the following.

1. Disconnect power at fuse or circuit breaker before installing or servicing.
2. Do not use outdoors.
3. Do not mount in hazardous locations, or near gas or electric heaters.
4. Do not let power cords touch hot surface.
5. Equipment should be mounted in locations and at heights where it will not be subjected to tampering by unauthorized personnel.
6. Do not use this equipment for other than intended use.
7. All servicing should be performed by a qualified only.

**SAVE THESE INSTRUCTIONS**

**Instruction**

1.Connect wires to DC3.6-9.6V supply in accordance with local and national code,yellow wire is for positive,bule wire is for negative.

2.Secure fixture to junction box with hardware provided.

**Model List and Ratings**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NO | Model List | Lamp Head | LED source | Lumen output |
| 1 | JLRH-1 | Single head | 1x1.0W | ≥100lm |
| 2 | JLRH-2 | Dual head | 2x1.0W | ≥200lm |

**Wiring Diagram**

|  |  |
| --- | --- |
| IMG_256 | IMG_256 |